(export (version D)
  (design
    (source F:/kicad-launchpad/testing/demos/test_xil_95108/carte_test.sch)
    (date "09/01/2014 18:43:28")
    (tool "eeschema (2014-01-08 BZR 4616)-product"))
  (components
    (comp (ref J2)
      (value DB9FEM)
      (libsource (lib carte_test-cache) (part DB9))
      (sheetpath (names /) (tstamps /))
      (tstamp 3ECDEBEA))
    (comp (ref D4)
      (value 1N4004)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /) (tstamps /))
      (tstamp 3ECDDCDD))
    (comp (ref C13)
      (value 10uF)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 3ECDDCAD))
    (comp (ref U6)
      (value LM318N)
      (libsource (lib linear) (part LM318N))
      (sheetpath (names /) (tstamps /))
      (tstamp 3ECDDB8B))
    (comp (ref R10)
      (value 75)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3ECDDB6D))
    (comp (ref R7)
      (value 1,1K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3ECDDB60))
    (comp (ref R6)
      (value 1,1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3ECDDB57))
    (comp (ref R9)
      (value 2,2K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3ECDDB4B))
    (comp (ref R8)
      (value 2,2K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3ECDDB43))
    (comp (ref C14)
      (value 10uF)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 3ECDDACB))
    (comp (ref P4)
      (value CONN_2X2)
      (libsource (lib carte_test-cache) (part CONN_2X2))
      (sheetpath (names /) (tstamps /))
      (tstamp 3ECB3F5E))
    (comp (ref J1)
      (value DB25)
      (libsource (lib carte_test-cache) (part DB25))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC4C60F))
    (comp (ref U2)
      (value XC95108PC84)
      (libsource (lib xilinx) (part XC95108PC84))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC230AD))
    (comp (ref R5)
      (value 4,7K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC8B978))
    (comp (ref R4)
      (value 4,7K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC8B970))
    (comp (ref SW2)
      (value SW_PUSH)
      (libsource (lib device) (part SW_PUSH))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC8B882))
    (comp (ref SW1)
      (value SW_PUSH)
      (libsource (lib device) (part SW_PUSH))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC8B876))
    (comp (ref D3)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC4D08F))
    (comp (ref R3)
      (value 330)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC4D082))
    (comp (ref D2)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 52CEE1D4))
    (comp (ref R2)
      (value 330)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52CEE1D3))
    (comp (ref C12)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC4C7DB))
    (comp (ref C7)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52CEE1C8))
    (comp (ref C11)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52CEE1C7))
    (comp (ref C10)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52CEE1C9))
    (comp (ref C8)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52CEE1CA))
    (comp (ref K1)
      (value CONN_3)
      (libsource (lib carte_test-cache) (part CONN_3))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC4C49F))
    (comp (ref U5)
      (value RAM_32KO)
      (libsource (lib memory) (part RAM_32KO))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC4C463))
    (comp (ref U4)
      (value 74HC04)
      (libsource (lib 74xx) (part 74HC04))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC4C318))
    (comp (ref P3)
      (value CONN_2)
      (libsource (lib carte_test-cache) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC2446D))
    (comp (ref C6)
      (value 47uF)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC243D6))
    (comp (ref D1)
      (value 1N4004)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC243C8))
    (comp (ref P2)
      (value CONN_3)
      (libsource (lib carte_test-cache) (part CONN_3))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC243AC))
    (comp (ref U3)
      (value LM7805)
      (libsource (lib regul) (part LM7805))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC2436D))
    (comp (ref C4)
      (value 22pF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC242AD))
    (comp (ref R1)
      (value 100K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC242C1))
    (comp (ref C5)
      (value 22pF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52CEE1C5))
    (comp (ref X1)
      (value 10MHz)
      (libsource (lib device) (part CRYSTAL))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC2428D))
    (comp (ref C3)
      (value 10uF)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC23DCD))
    (comp (ref C2)
      (value 10uF)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC23B98))
    (comp (ref C1)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC23ABA))
    (comp (ref U1)
      (value TDA8702)
      (libsource (lib adc-dac) (part TDA8702))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EC238E5)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP)
      (aliases
        (alias CAPAPOL))
      (description "Condensateur polarise")
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CRYSTAL)
      (fields
        (field (name Reference) X)
        (field (name Value) CRYSTAL))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part DIODE)
      (description "Diode simple")
      (footprints
        (fp D?)
        (fp S*))
      (fields
        (field (name Reference) D)
        (field (name Value) DIODE))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part SW_PUSH)
      (description "Push Button")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib linear) (part LM318N)
      (description "ampli Op")
      (docs op_amps/LM118.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) LM318N))
      (pins
        (pin (num 1) (name FIN2) (type passive))
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V-) (type power_in))
        (pin (num 5) (name FOUT) (type passive))
        (pin (num 6) (name OUT) (type output))
        (pin (num 7) (name V+) (type power_in))
        (pin (num 8) (name FIN1) (type passive))))
    (libpart (lib regul) (part 7805)
      (aliases
        (alias LM7805)
        (alias LM7812)
        (alias 78L05))
      (description "Linear Regulator +5V")
      (docs regulator\lm78xx.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) 7805))
      (pins
        (pin (num GND) (name GND) (type input))
        (pin (num VI) (name VI) (type input))
        (pin (num VO) (name VO) (type power_out))))
    (libpart (lib 74xx) (part 74HCT04)
      (aliases
        (alias 74HC14)
        (alias 74HC04)
        (alias 74LS14))
      (description "Hex Inverseur")
      (fields
        (field (name Reference) U)
        (field (name Value) 74HCT04))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type output))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name ~) (type output))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type output))
        (pin (num 11) (name ~) (type input))
        (pin (num 12) (name ~) (type output))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib adc-dac) (part TDA8702)
      (description "Video DAC (32 MHz)")
      (docs philips/tda8702.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) TDA8702))
      (pins
        (pin (num 1) (name VREF) (type BiDi))
        (pin (num 2) (name AGND) (type power_in))
        (pin (num 3) (name DB2) (type input))
        (pin (num 4) (name DB3) (type input))
        (pin (num 5) (name Clock) (type input))
        (pin (num 6) (name DGND) (type power_in))
        (pin (num 7) (name DB7) (type input))
        (pin (num 8) (name DB6) (type input))
        (pin (num 9) (name DB5) (type input))
        (pin (num 10) (name DB4) (type input))
        (pin (num 11) (name DB1) (type input))
        (pin (num 12) (name DB0) (type input))
        (pin (num 13) (name VCCD) (type power_in))
        (pin (num 14) (name VOUT) (type output))
        (pin (num 15) (name VOUT) (type output))
        (pin (num 16) (name VCCA) (type power_in))))
    (libpart (lib memory) (part RAM_32KO)
      (description "RAM 32 Ko")
      (fields
        (field (name Reference) U)
        (field (name Value) RAM_32KO))
      (pins
        (pin (num 1) (name A14) (type input))
        (pin (num 2) (name A12) (type input))
        (pin (num 3) (name A7) (type input))
        (pin (num 4) (name A6) (type input))
        (pin (num 5) (name A5) (type input))
        (pin (num 6) (name A4) (type input))
        (pin (num 7) (name A3) (type input))
        (pin (num 8) (name A2) (type input))
        (pin (num 9) (name A1) (type input))
        (pin (num 10) (name A0) (type input))
        (pin (num 11) (name D0) (type 3state))
        (pin (num 12) (name D1) (type 3state))
        (pin (num 13) (name D2) (type 3state))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name D3) (type 3state))
        (pin (num 16) (name D4) (type 3state))
        (pin (num 17) (name D5) (type 3state))
        (pin (num 18) (name D6) (type 3state))
        (pin (num 19) (name D7) (type 3state))
        (pin (num 20) (name CS) (type input))
        (pin (num 21) (name A10) (type input))
        (pin (num 22) (name OE) (type input))
        (pin (num 23) (name A11) (type input))
        (pin (num 24) (name A9) (type input))
        (pin (num 25) (name A8) (type input))
        (pin (num 26) (name A13) (type input))
        (pin (num 27) (name WE) (type input))
        (pin (num 28) (name VCC) (type power_in))))
    (libpart (lib xilinx) (part XC95108PC84)
      (docs xilinx/xc95108.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) XC95108PC84))
      (pins
        (pin (num 1) (name P1) (type BiDi))
        (pin (num 2) (name P2) (type BiDi))
        (pin (num 3) (name P3) (type BiDi))
        (pin (num 4) (name P4) (type BiDi))
        (pin (num 5) (name P5) (type BiDi))
        (pin (num 6) (name P6) (type BiDi))
        (pin (num 7) (name P7) (type BiDi))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name I/O/GCK1) (type BiDi))
        (pin (num 10) (name I/O/GCK2) (type BiDi))
        (pin (num 11) (name P11) (type BiDi))
        (pin (num 12) (name I/O/GCK3) (type BiDi))
        (pin (num 13) (name P13) (type BiDi))
        (pin (num 14) (name P14) (type BiDi))
        (pin (num 15) (name P15) (type BiDi))
        (pin (num 16) (name GND) (type power_in))
        (pin (num 17) (name P17) (type BiDi))
        (pin (num 18) (name P18) (type BiDi))
        (pin (num 19) (name P19) (type BiDi))
        (pin (num 20) (name P20) (type BiDi))
        (pin (num 21) (name P21) (type BiDi))
        (pin (num 22) (name VCCIO) (type power_in))
        (pin (num 23) (name P23) (type BiDi))
        (pin (num 24) (name P24) (type BiDi))
        (pin (num 25) (name P25) (type BiDi))
        (pin (num 26) (name P26) (type BiDi))
        (pin (num 27) (name GND) (type power_in))
        (pin (num 28) (name TDI) (type input))
        (pin (num 29) (name TMS) (type input))
        (pin (num 30) (name TCK) (type input))
        (pin (num 31) (name P31) (type BiDi))
        (pin (num 32) (name P32) (type BiDi))
        (pin (num 33) (name P33) (type BiDi))
        (pin (num 34) (name P34) (type BiDi))
        (pin (num 35) (name P35) (type BiDi))
        (pin (num 36) (name P36) (type BiDi))
        (pin (num 37) (name P37) (type BiDi))
        (pin (num 38) (name VCC) (type power_in))
        (pin (num 39) (name P39) (type BiDi))
        (pin (num 40) (name P40) (type BiDi))
        (pin (num 41) (name P41) (type BiDi))
        (pin (num 42) (name GND) (type power_in))
        (pin (num 43) (name P43) (type BiDi))
        (pin (num 44) (name P44) (type BiDi))
        (pin (num 45) (name P45) (type BiDi))
        (pin (num 46) (name P46) (type BiDi))
        (pin (num 47) (name P47) (type BiDi))
        (pin (num 48) (name P48) (type BiDi))
        (pin (num 49) (name GND) (type power_in))
        (pin (num 50) (name P50) (type BiDi))
        (pin (num 51) (name P51) (type BiDi))
        (pin (num 52) (name P52) (type BiDi))
        (pin (num 53) (name P53) (type BiDi))
        (pin (num 54) (name P54) (type BiDi))
        (pin (num 55) (name P55) (type BiDi))
        (pin (num 56) (name P56) (type BiDi))
        (pin (num 57) (name P57) (type BiDi))
        (pin (num 58) (name P58) (type BiDi))
        (pin (num 59) (name TDO) (type output))
        (pin (num 60) (name GND) (type power_in))
        (pin (num 61) (name P61) (type BiDi))
        (pin (num 62) (name P62) (type BiDi))
        (pin (num 63) (name P63) (type BiDi))
        (pin (num 64) (name VCCIO) (type power_in))
        (pin (num 65) (name P65) (type BiDi))
        (pin (num 66) (name P66) (type BiDi))
        (pin (num 67) (name P67) (type BiDi))
        (pin (num 68) (name P68) (type BiDi))
        (pin (num 69) (name P69) (type BiDi))
        (pin (num 70) (name P70) (type BiDi))
        (pin (num 71) (name P71) (type BiDi))
        (pin (num 72) (name P72) (type BiDi))
        (pin (num 73) (name VCC) (type power_in))
        (pin (num 74) (name I/O/GSR) (type BiDi))
        (pin (num 75) (name P75) (type BiDi))
        (pin (num 76) (name I/O/GTS1) (type BiDi))
        (pin (num 77) (name I/O/GTS2) (type BiDi))
        (pin (num 78) (name VCC) (type power_in))
        (pin (num 79) (name P79) (type BiDi))
        (pin (num 80) (name P80) (type BiDi))
        (pin (num 81) (name P81) (type BiDi))
        (pin (num 82) (name P82) (type BiDi))
        (pin (num 83) (name P83) (type BiDi))
        (pin (num 84) (name P84) (type BiDi))))
    (libpart (lib carte_test-cache) (part CONN_2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib carte_test-cache) (part CONN_2X2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2X2))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib carte_test-cache) (part CONN_3)
      (fields
        (field (name Reference) K)
        (field (name Value) CONN_3))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib carte_test-cache) (part DB25)
      (fields
        (field (name Reference) J)
        (field (name Value) DB25))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))
        (pin (num 10) (name 10) (type passive))
        (pin (num 11) (name 11) (type passive))
        (pin (num 12) (name 12) (type passive))
        (pin (num 13) (name 13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))))
    (libpart (lib carte_test-cache) (part DB9)
      (fields
        (field (name Reference) J)
        (field (name Value) DB9))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive)))))
  (libraries
    (library (logical device)
      (uri F:\kicad\share\library\device.lib))
    (library (logical linear)
      (uri F:\kicad\share\library\linear.lib))
    (library (logical regul)
      (uri F:\kicad\share\library\regul.lib))
    (library (logical 74xx)
      (uri F:\kicad\share\library\74xx.lib))
    (library (logical memory)
      (uri F:\kicad\share\library\memory.lib))
    (library (logical adc-dac)
      (uri F:\kicad\share\library\adc-dac.lib))
    (library (logical xilinx)
      (uri F:\kicad\share\library\xilinx.lib))
    (library (logical carte_test-cache)
      (uri F:\kicad-launchpad\testing\demos\test_xil_95108\carte_test-cache.lib)))
  (nets
    (net (code 1) (name GND)
      (node (ref P4) (pin 3))
      (node (ref P4) (pin 1))
      (node (ref J1) (pin 20))
      (node (ref U2) (pin 8))
      (node (ref P2) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref U2) (pin 60))
      (node (ref R6) (pin 2))
      (node (ref C13) (pin 1))
      (node (ref J2) (pin 9))
      (node (ref J2) (pin 8))
      (node (ref J2) (pin 7))
      (node (ref J2) (pin 6))
      (node (ref J1) (pin 19))
      (node (ref J1) (pin 25))
      (node (ref J1) (pin 23))
      (node (ref J1) (pin 22))
      (node (ref J1) (pin 21))
      (node (ref J1) (pin 18))
      (node (ref U1) (pin 2))
      (node (ref U4) (pin 7))
      (node (ref U4) (pin 9))
      (node (ref U1) (pin 6))
      (node (ref P3) (pin 2))
      (node (ref U4) (pin 13))
      (node (ref C4) (pin 2))
      (node (ref U4) (pin 11))
      (node (ref U4) (pin 5))
      (node (ref C6) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref J1) (pin 24))
      (node (ref C3) (pin 2))
      (node (ref U3) (pin GND))
      (node (ref C1) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref D3) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref U2) (pin 16))
      (node (ref U5) (pin 14))
      (node (ref U2) (pin 42))
      (node (ref U2) (pin 27))
      (node (ref U2) (pin 49))
      (node (ref C7) (pin 2))
      (node (ref SW1) (pin 2))
      (node (ref SW2) (pin 2))
      (node (ref C12) (pin 2)))
    (net (code 2) (name /MA3)
      (node (ref U2) (pin 25))
      (node (ref U5) (pin 15)))
    (net (code 3) (name /MA2)
      (node (ref U5) (pin 13))
      (node (ref U2) (pin 26)))
    (net (code 4) (name /MA1)
      (node (ref U5) (pin 12))
      (node (ref U2) (pin 32)))
    (net (code 5) (name /MA0)
      (node (ref U5) (pin 11))
      (node (ref U2) (pin 33)))
    (net (code 6) (name VCC)
      (node (ref K1) (pin 1))
      (node (ref U4) (pin 14))
      (node (ref U3) (pin VO))
      (node (ref U1) (pin 16))
      (node (ref J2) (pin 1))
      (node (ref U2) (pin 22))
      (node (ref U2) (pin 78))
      (node (ref U2) (pin 38))
      (node (ref R4) (pin 1))
      (node (ref U5) (pin 28))
      (node (ref R5) (pin 1))
      (node (ref U1) (pin 13))
      (node (ref C8) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref U2) (pin 64))
      (node (ref U2) (pin 73))
      (node (ref C12) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref C11) (pin 1)))
    (net (code 7) (name "Net-(K1-Pad2)")
      (node (ref U5) (pin 1))
      (node (ref K1) (pin 2)))
    (net (code 8) (name "Net-(U4-Pad6)")
      (node (ref U4) (pin 6)))
    (net (code 9) (name "Net-(U4-Pad12)")
      (node (ref U4) (pin 12)))
    (net (code 10) (name "Net-(U4-Pad10)")
      (node (ref U4) (pin 10)))
    (net (code 11) (name "Net-(U4-Pad8)")
      (node (ref U4) (pin 8)))
    (net (code 12) (name /MA4)
      (node (ref U5) (pin 16))
      (node (ref U2) (pin 24)))
    (net (code 13) (name /XIN/CLK)
      (node (ref U4) (pin 4))
      (node (ref U2) (pin 12)))
    (net (code 14) (name /MD9)
      (node (ref U5) (pin 24))
      (node (ref U2) (pin 47)))
    (net (code 15) (name /MD8)
      (node (ref U2) (pin 51))
      (node (ref U5) (pin 25)))
    (net (code 16) (name /MD7)
      (node (ref U2) (pin 52))
      (node (ref U5) (pin 3)))
    (net (code 17) (name /MD6)
      (node (ref U5) (pin 4))
      (node (ref U2) (pin 50)))
    (net (code 18) (name /MD5)
      (node (ref U5) (pin 5))
      (node (ref U2) (pin 48)))
    (net (code 19) (name /MD4)
      (node (ref U2) (pin 46))
      (node (ref U5) (pin 6)))
    (net (code 20) (name /MD3)
      (node (ref U5) (pin 7))
      (node (ref U2) (pin 44)))
    (net (code 21) (name /MD2)
      (node (ref U2) (pin 40))
      (node (ref U5) (pin 8)))
    (net (code 22) (name /MD1)
      (node (ref U2) (pin 37))
      (node (ref U5) (pin 9)))
    (net (code 23) (name /MD0)
      (node (ref U5) (pin 10))
      (node (ref U2) (pin 35)))
    (net (code 24) (name /MD10)
      (node (ref U2) (pin 41))
      (node (ref U5) (pin 21)))
    (net (code 25) (name /PAR_AUX6/ACK)
      (node (ref U2) (pin 79))
      (node (ref J1) (pin 10)))
    (net (code 26) (name /PAR_AUX2/AUTOLF*)
      (node (ref U2) (pin 11))
      (node (ref J1) (pin 14)))
    (net (code 27) (name /PARBUS7)
      (node (ref U2) (pin 82))
      (node (ref J1) (pin 9)))
    (net (code 28) (name /PARBUS6)
      (node (ref U2) (pin 81))
      (node (ref J1) (pin 8)))
    (net (code 29) (name /PARBUS5)
      (node (ref U2) (pin 83))
      (node (ref J1) (pin 7)))
    (net (code 30) (name /PARBUS4)
      (node (ref U2) (pin 84))
      (node (ref J1) (pin 6)))
    (net (code 31) (name /PARBUS3)
      (node (ref U2) (pin 3))
      (node (ref J1) (pin 5)))
    (net (code 32) (name /PARBUS2)
      (node (ref U2) (pin 5))
      (node (ref J1) (pin 4)))
    (net (code 33) (name /PARBUS1)
      (node (ref U2) (pin 7))
      (node (ref J1) (pin 3)))
    (net (code 34) (name /PARBUS0)
      (node (ref J1) (pin 2))
      (node (ref U2) (pin 10)))
    (net (code 35) (name /MD13)
      (node (ref U5) (pin 26))
      (node (ref U2) (pin 53)))
    (net (code 36) (name /MD12)
      (node (ref U2) (pin 55))
      (node (ref U5) (pin 2)))
    (net (code 37) (name /MD11)
      (node (ref U2) (pin 45))
      (node (ref U5) (pin 23)))
    (net (code 38) (name /R/W-A14)
      (node (ref U5) (pin 27))
      (node (ref U2) (pin 54)))
    (net (code 39) (name /OEMEM)
      (node (ref U5) (pin 22))
      (node (ref U2) (pin 43)))
    (net (code 40) (name /CSMEM)
      (node (ref U5) (pin 20))
      (node (ref U2) (pin 39)))
    (net (code 41) (name /MD14)
      (node (ref K1) (pin 3))
      (node (ref U2) (pin 56)))
    (net (code 42) (name /MA7)
      (node (ref U2) (pin 36))
      (node (ref U5) (pin 19)))
    (net (code 43) (name /MA6)
      (node (ref U2) (pin 34))
      (node (ref U5) (pin 18)))
    (net (code 44) (name /MA5)
      (node (ref U2) (pin 31))
      (node (ref U5) (pin 17)))
    (net (code 45) (name /DCLK)
      (node (ref U2) (pin 67))
      (node (ref U1) (pin 5)))
    (net (code 46) (name /DAT7)
      (node (ref U1) (pin 7))
      (node (ref U2) (pin 62)))
    (net (code 47) (name /DAT6)
      (node (ref U2) (pin 58))
      (node (ref U1) (pin 8)))
    (net (code 48) (name /DAT5)
      (node (ref U1) (pin 9))
      (node (ref U2) (pin 61)))
    (net (code 49) (name /DAT4)
      (node (ref U1) (pin 10))
      (node (ref U2) (pin 63)))
    (net (code 50) (name /DAT3)
      (node (ref U2) (pin 68))
      (node (ref U1) (pin 4)))
    (net (code 51) (name /TDO)
      (node (ref J2) (pin 2))
      (node (ref U2) (pin 59)))
    (net (code 52) (name /DAT2)
      (node (ref U1) (pin 3))
      (node (ref U2) (pin 70)))
    (net (code 53) (name "Net-(C2-Pad1)")
      (node (ref U1) (pin 14))
      (node (ref C2) (pin 1)))
    (net (code 54) (name "Net-(C2-Pad2)")
      (node (ref R9) (pin 2))
      (node (ref C2) (pin 2)))
    (net (code 55) (name "Net-(C1-Pad1)")
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 1)))
    (net (code 56) (name "Net-(C14-Pad1)")
      (node (ref C14) (pin 1))
      (node (ref U1) (pin 15)))
    (net (code 57) (name /DAT1)
      (node (ref U1) (pin 11))
      (node (ref U2) (pin 66)))
    (net (code 58) (name /DAT0)
      (node (ref U1) (pin 12))
      (node (ref U2) (pin 69)))
    (net (code 59) (name "Net-(C4-Pad1)")
      (node (ref X1) (pin 2))
      (node (ref U4) (pin 3))
      (node (ref U4) (pin 2))
      (node (ref R1) (pin 1))
      (node (ref C4) (pin 1)))
    (net (code 60) (name "Net-(C5-Pad1)")
      (node (ref U4) (pin 1))
      (node (ref R1) (pin 2))
      (node (ref C5) (pin 1))
      (node (ref X1) (pin 1)))
    (net (code 61) (name "Net-(D1-Pad1)")
      (node (ref P2) (pin 1))
      (node (ref D1) (pin 1)))
    (net (code 62) (name "Net-(D4-Pad2)")
      (node (ref D4) (pin 2))
      (node (ref P2) (pin 3)))
    (net (code 63) (name /PAR_AUX8/SELECT)
      (node (ref J1) (pin 17))
      (node (ref U2) (pin 4)))
    (net (code 64) (name /PIN_TEST1)
      (node (ref U2) (pin 2))
      (node (ref P4) (pin 4)))
    (net (code 65) (name /PIN_TEST0)
      (node (ref U2) (pin 1))
      (node (ref P4) (pin 2)))
    (net (code 66) (name /PAR_AUX7/INIT)
      (node (ref U2) (pin 6))
      (node (ref J1) (pin 16)))
    (net (code 67) (name "Net-(U2-Pad20)")
      (node (ref U2) (pin 20)))
    (net (code 68) (name "Net-(C14-Pad2)")
      (node (ref C14) (pin 2))
      (node (ref R8) (pin 2)))
    (net (code 69) (name "Net-(U2-Pad23)")
      (node (ref U2) (pin 23)))
    (net (code 70) (name "Net-(U2-Pad21)")
      (node (ref U2) (pin 21)))
    (net (code 71) (name "Net-(U2-Pad19)")
      (node (ref U2) (pin 19)))
    (net (code 72) (name "Net-(U2-Pad18)")
      (node (ref U2) (pin 18)))
    (net (code 73) (name "Net-(U2-Pad17)")
      (node (ref U2) (pin 17)))
    (net (code 74) (name "Net-(U2-Pad15)")
      (node (ref U2) (pin 15)))
    (net (code 75) (name "Net-(U2-Pad14)")
      (node (ref U2) (pin 14)))
    (net (code 76) (name /TMS)
      (node (ref J2) (pin 5))
      (node (ref U2) (pin 29)))
    (net (code 77) (name -12V)
      (node (ref U6) (pin 4))
      (node (ref C13) (pin 2))
      (node (ref D4) (pin 1)))
    (net (code 78) (name /TCK)
      (node (ref J2) (pin 4))
      (node (ref U2) (pin 30)))
    (net (code 79) (name /SW0)
      (node (ref U2) (pin 72))
      (node (ref SW1) (pin 1))
      (node (ref R5) (pin 2)))
    (net (code 80) (name /TDI)
      (node (ref U2) (pin 28))
      (node (ref J2) (pin 3)))
    (net (code 81) (name "Net-(P3-Pad1)")
      (node (ref P3) (pin 1))
      (node (ref R10) (pin 1)))
    (net (code 82) (name "Net-(R10-Pad2)")
      (node (ref R10) (pin 2))
      (node (ref R7) (pin 1))
      (node (ref U6) (pin 6)))
    (net (code 83) (name "Net-(U6-Pad1)")
      (node (ref U6) (pin 1)))
    (net (code 84) (name "Net-(R6-Pad1)")
      (node (ref U6) (pin 3))
      (node (ref R6) (pin 1))
      (node (ref R9) (pin 1)))
    (net (code 85) (name "Net-(U6-Pad5)")
      (node (ref U6) (pin 5)))
    (net (code 86) (name +12V)
      (node (ref D1) (pin 2))
      (node (ref C6) (pin 1))
      (node (ref U3) (pin VI))
      (node (ref U6) (pin 7)))
    (net (code 87) (name "Net-(U6-Pad8)")
      (node (ref U6) (pin 8)))
    (net (code 88) (name "Net-(R7-Pad2)")
      (node (ref U6) (pin 2))
      (node (ref R8) (pin 1))
      (node (ref R7) (pin 2)))
    (net (code 89) (name /LED1)
      (node (ref U2) (pin 76))
      (node (ref R2) (pin 2)))
    (net (code 90) (name "Net-(D3-Pad1)")
      (node (ref D3) (pin 1))
      (node (ref R3) (pin 1)))
    (net (code 91) (name "Net-(D2-Pad1)")
      (node (ref D2) (pin 1))
      (node (ref R2) (pin 1)))
    (net (code 92) (name /SW1)
      (node (ref R4) (pin 2))
      (node (ref U2) (pin 71))
      (node (ref SW2) (pin 1)))
    (net (code 93) (name /PAR_AUX1/ERROR*)
      (node (ref J1) (pin 15))
      (node (ref U2) (pin 9)))
    (net (code 94) (name /PAR_AUX0/STROBE*)
      (node (ref U2) (pin 13))
      (node (ref J1) (pin 1)))
    (net (code 95) (name /PAR_AUX5/BUSY*)
      (node (ref U2) (pin 80))
      (node (ref J1) (pin 11)))
    (net (code 96) (name /PAR_AUX4/PE)
      (node (ref J1) (pin 12))
      (node (ref U2) (pin 77)))
    (net (code 97) (name /PAR_AUX3/SELECT*)
      (node (ref J1) (pin 13))
      (node (ref U2) (pin 75)))
    (net (code 98) (name /LED2)
      (node (ref U2) (pin 74))
      (node (ref R3) (pin 2)))
    (net (code 99) (name "Net-(U2-Pad65)")
      (node (ref U2) (pin 65)))
    (net (code 100) (name "Net-(U2-Pad57)")
      (node (ref U2) (pin 57)))))