G04 Test layer rotation 1 *
G04 Quarter star should be rotated 45 degrees counterclockwise, pointing*
G04   the center line straight up *
G04 Handcoded by Julian Lamb *
%MOIN*%
%FSLAX23Y23*%
%RO45.0*%
%ADD10C,0.025*%

G04 Quarter star *
X1000Y0D02*
G54D10*
X2000Y0D01*

X1000Y0D02*
G54D10*
X2000Y1000D01*

X1000Y0D02*
G54D10*
X1000Y1000D01*

M02*
