Cmp-Mod V01 Created by Cvpcb (2014-07-04 BZR 4974)-product   date = 05/07/2014 20:15:53

BeginCmp
TimeStamp = /48553E53/442A5056;
Reference = C1;
ValeurCmp = 100uF;
IdModule  = discret:CP10;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A501D;
Reference = C2;
ValeurCmp = 220uF;
IdModule  = discret:CP10;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A584C;
Reference = C3;
ValeurCmp = 22uF/25V;
IdModule  = discret:CP8;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A5F61;
Reference = C4;
ValeurCmp = 0;
IdModule  = discret:C1-1;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A58B1;
Reference = C5;
ValeurCmp = 10nF;
IdModule  = discret:C1-1;
EndCmp

BeginCmp
TimeStamp = /48553E7C/442AA12B;
Reference = C6;
ValeurCmp = 100nF;
IdModule  = discret:C1-1;
EndCmp

BeginCmp
TimeStamp = /48553E7C/442AA145;
Reference = C7;
ValeurCmp = 100nF;
IdModule  = discret:C1-1;
EndCmp

BeginCmp
TimeStamp = /48553E7C/4639BE2C;
Reference = C8;
ValeurCmp = 100nF;
IdModule  = discret:C1-1;
EndCmp

BeginCmp
TimeStamp = /48553E53/464AD280;
Reference = C9;
ValeurCmp = 22OnF;
IdModule  = discret:C1-1;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A500B;
Reference = D1;
ValeurCmp = 1N4004;
IdModule  = discret:D5;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4D1B;
Reference = D2;
ValeurCmp = BAT43;
IdModule  = discret:D3;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4D25;
Reference = D3;
ValeurCmp = BAT43;
IdModule  = discret:D3;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4D5C;
Reference = D4;
ValeurCmp = BAT43;
IdModule  = discret:D3;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4D5D;
Reference = D5;
ValeurCmp = BAT43;
IdModule  = discret:D3;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4D64;
Reference = D6;
ValeurCmp = BAT43;
IdModule  = discret:D3;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4D65;
Reference = D7;
ValeurCmp = BAT43;
IdModule  = discret:D3;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4F5D;
Reference = D8;
ValeurCmp = RED-LED;
IdModule  = discret:LEDV;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A5084;
Reference = D9;
ValeurCmp = GREEN-LED;
IdModule  = discret:LEDV;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A6026;
Reference = D10;
ValeurCmp = SCHOTTKY;
IdModule  = discret:D5;
EndCmp

BeginCmp
TimeStamp = /48553E53/4639BA28;
Reference = D11;
ValeurCmp = BAT43;
IdModule  = discret:D3;
EndCmp

BeginCmp
TimeStamp = /48553E53/4639B9EA;
Reference = D12;
ValeurCmp = YELLOW-LED;
IdModule  = discret:LEDV;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4C93;
Reference = J1;
ValeurCmp = DB9-FEMAL;
IdModule  = connect:DB9FC;
EndCmp

BeginCmp
TimeStamp = /48553E53/4639BAF8;
Reference = JP1;
ValeurCmp = JUMPER;
IdModule  = pin_array:PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A57BE;
Reference = L1;
ValeurCmp = 22uH;
IdModule  = inductors:INDUCTOR_V;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4FE7;
Reference = P1;
ValeurCmp = CONN_2;
IdModule  = connect:bornier2;
EndCmp

BeginCmp
TimeStamp = /48553E7C/4436967E;
Reference = P2;
ValeurCmp = SUPP28;
IdModule  = 28DIP-ELL300;
EndCmp

BeginCmp
TimeStamp = /48553E7C/442A88ED;
Reference = P3;
ValeurCmp = SUPP40;
IdModule  = 40DIP-ELL600;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4EB9;
Reference = Q1;
ValeurCmp = BC237;
IdModule  = discret:TO92;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4F30;
Reference = Q2;
ValeurCmp = BC307;
IdModule  = discret:TO92;
EndCmp

BeginCmp
TimeStamp = /48553E53/4639B996;
Reference = Q3;
ValeurCmp = BC307;
IdModule  = discret:TO92;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4CF4;
Reference = R1;
ValeurCmp = 10K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4CFB;
Reference = R2;
ValeurCmp = 10K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4D5A;
Reference = R3;
ValeurCmp = 10K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4D5B;
Reference = R4;
ValeurCmp = 10K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4D62;
Reference = R5;
ValeurCmp = 10K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4D63;
Reference = R6;
ValeurCmp = 10K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4F2A;
Reference = R7;
ValeurCmp = 10K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4D92;
Reference = R8;
ValeurCmp = 1K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4F52;
Reference = R9;
ValeurCmp = 2.2K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A5F83;
Reference = R10;
ValeurCmp = 5,1K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4F23;
Reference = R11;
ValeurCmp = 22K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4D85;
Reference = R12;
ValeurCmp = 470;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4D8D;
Reference = R13;
ValeurCmp = 470;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A5083;
Reference = R14;
ValeurCmp = 470;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A58D7;
Reference = R15;
ValeurCmp = 6.2K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A58DC;
Reference = R16;
ValeurCmp = 62K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A50BF;
Reference = R17;
ValeurCmp = 22K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/44369638;
Reference = R18;
ValeurCmp = 220;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/4639B9B0;
Reference = R19;
ValeurCmp = 2.2K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/4639B9B3;
Reference = R20;
ValeurCmp = 2.2K;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/4639B9E9;
Reference = R21;
ValeurCmp = 470;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /48553E53/443D0101;
Reference = RV1;
ValeurCmp = 1K;
IdModule  = discret:RV2X4;
EndCmp

BeginCmp
TimeStamp = /48553E7C/442A87F7;
Reference = U1;
ValeurCmp = 24Cxx;
IdModule  = dip_sockets:DIP-8__300_ELL;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A4D6B;
Reference = U2;
ValeurCmp = 74HC125;
IdModule  = dip_sockets:DIP-14__300_ELL;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A504A;
Reference = U3;
ValeurCmp = 7805;
IdModule  = discret:LM78XX;
EndCmp

BeginCmp
TimeStamp = /48553E53/442A5E20;
Reference = U4;
ValeurCmp = LT1373;
IdModule  = dip_sockets:DIP-8__300_ELL;
EndCmp

BeginCmp
TimeStamp = /48553E7C/442A81A7;
Reference = U5;
ValeurCmp = PIC_18_PINS;
IdModule  = dip_sockets:DIP-18__300_ELL;
EndCmp

BeginCmp
TimeStamp = /48553E7C/442A81A5;
Reference = U6;
ValeurCmp = PIC_8_PINS;
IdModule  = dip_sockets:DIP-8__300_ELL;
EndCmp

EndListe
