Cmp-Mod V01 Created by CvPcb (2013-08-20 BZR 4294)-product date = 21/08/2013 18:12:43

BeginCmp
TimeStamp = /322D3011;
Reference = BUS1;
ValeurCmp = BUSPC;
IdModule  = BUS_PC;
EndCmp

BeginCmp
TimeStamp = /32307DE2;
Reference = C1;
ValeurCmp = 47uF;
IdModule  = CP6;
EndCmp

BeginCmp
TimeStamp = /32307ECF;
Reference = C2;
ValeurCmp = 47pF;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /32307ED4;
Reference = C3;
ValeurCmp = 47pF;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /32307DCF;
Reference = C4;
ValeurCmp = 47uF;
IdModule  = CP6;
EndCmp

BeginCmp
TimeStamp = /32307DCA;
Reference = C5;
ValeurCmp = 47uF;
IdModule  = CP6;
EndCmp

BeginCmp
TimeStamp = /32307DC0;
Reference = C6;
ValeurCmp = 47uF;
IdModule  = CP6;
EndCmp

BeginCmp
TimeStamp = /322D32AC;
Reference = D1;
ValeurCmp = LED;
IdModule  = LEDV;
EndCmp

BeginCmp
TimeStamp = /322D32BE;
Reference = D2;
ValeurCmp = LED;
IdModule  = LEDV;
EndCmp

BeginCmp
TimeStamp = /32568D1E;
Reference = JP1;
ValeurCmp = CONN_8X2;
IdModule  = pin_array_8x2;
EndCmp

BeginCmp
TimeStamp = /3256759C;
Reference = P1;
ValeurCmp = DB25FEMELLE;
IdModule  = DB25FC;
EndCmp

BeginCmp
TimeStamp = /32307EA1;
Reference = R1;
ValeurCmp = 100K;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /32307EAA;
Reference = R2;
ValeurCmp = 1K;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /324002E6;
Reference = R3;
ValeurCmp = 10K;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /322D3295;
Reference = R4;
ValeurCmp = 330;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /322D32A0;
Reference = R5;
ValeurCmp = 330;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /325679C1;
Reference = RR1;
ValeurCmp = 9x1K;
IdModule  = r_pack9;
EndCmp

BeginCmp
TimeStamp = /322D31F4;
Reference = U1;
ValeurCmp = 74LS245;
IdModule  = DIP-20__300;
EndCmp

BeginCmp
TimeStamp = /322D35B4;
Reference = U2;
ValeurCmp = 74LS688;
IdModule  = DIP-20__300;
EndCmp

BeginCmp
TimeStamp = /4A087146;
Reference = U3;
ValeurCmp = 74LS541;
IdModule  = DIP-20__300;
EndCmp

BeginCmp
TimeStamp = /3240023F;
Reference = U5;
ValeurCmp = 628128;
IdModule  = DIP-32__600;
EndCmp

BeginCmp
TimeStamp = /322D321C;
Reference = U8;
ValeurCmp = EP600;
IdModule  = DIP-24__300;
EndCmp

BeginCmp
TimeStamp = /322D32FA;
Reference = U9;
ValeurCmp = 4003APG120;
IdModule  = PGA120;
EndCmp

BeginCmp
TimeStamp = /32307EC0;
Reference = X1;
ValeurCmp = 8MHz;
IdModule  = HC-18UH;
EndCmp

EndListe
