Cmp-Mod V01 Created by Cvpcb (2014-07-29 BZR 5035)-product   date = 30/07/2014 13:09:03

BeginCmp
TimeStamp = /46237F50;
Reference = ABRT_SW1;
ValeurCmp = SW_PUSH;
IdModule  = discret:SW_PUSH_SMALL;
EndCmp

BeginCmp
TimeStamp = /46238965;
Reference = ALLPST1;
ValeurCmp = CONN_1;
IdModule  = connect:PINTST;
EndCmp

BeginCmp
TimeStamp = /461BAF4F;
Reference = BDM_EN1;
ValeurCmp = JUMPER;
IdModule  = pin_array:PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /461BAEE7;
Reference = BDM_PORT1;
ValeurCmp = CONN_13X2;
IdModule  = pin_array:pin_array_13x2;
EndCmp

BeginCmp
TimeStamp = /462389BC;
Reference = C1;
ValeurCmp = 10pF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /462389C0;
Reference = C2;
ValeurCmp = 10pF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46238468;
Reference = C3;
ValeurCmp = 1nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46161CB5;
Reference = C4;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46161CB8;
Reference = C5;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BB5E5;
Reference = C6;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46161CD3;
Reference = C7;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46161CD4;
Reference = C8;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46161CD7;
Reference = C9;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46161CD8;
Reference = C10;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46161CD9;
Reference = C11;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46161CDA;
Reference = C12;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46237DF9;
Reference = C14;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46237E36;
Reference = C15;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /462382CE;
Reference = C16;
ValeurCmp = 10uF;
IdModule  = lib_smd:SM1206POL;
EndCmp

BeginCmp
TimeStamp = /46161D3C;
Reference = C17;
ValeurCmp = 100uF;
IdModule  = lib_smd:SM1206POL;
EndCmp

BeginCmp
TimeStamp = /46238286;
Reference = C18;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BE364;
Reference = C20;
ValeurCmp = 1nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BE35C;
Reference = C21;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B365;
Reference = C22;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B33B;
Reference = C23;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B354;
Reference = C24;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B35B;
Reference = C25;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/46546CA6;
Reference = C26;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B486;
Reference = C27;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4C7;
Reference = C28;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4C4;
Reference = C30;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4C5;
Reference = C31;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4C6;
Reference = C32;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4CA;
Reference = C33;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4653FFFE;
Reference = C34;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4D6;
Reference = C35;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4D8;
Reference = C36;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/465306B1;
Reference = C38;
ValeurCmp = 10uF;
IdModule  = discret:C2V8;
EndCmp

BeginCmp
TimeStamp = /47D80202/465305FE;
Reference = C40;
ValeurCmp = 220uF;
IdModule  = discret:C2V8;
EndCmp

BeginCmp
TimeStamp = /47D80202/465306F6;
Reference = C41;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652A9D3;
Reference = C43;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4D7;
Reference = C44;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4DC;
Reference = C45;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4D9;
Reference = C46;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BB2;
Reference = C51;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BB3;
Reference = C52;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BB4;
Reference = C53;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BB5;
Reference = C54;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BAE;
Reference = C55;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BAF;
Reference = C56;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BB0;
Reference = C57;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BB1;
Reference = C58;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BBA;
Reference = C59;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BBB;
Reference = C60;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BBC;
Reference = C61;
ValeurCmp = 100nF;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652BFF1;
Reference = CAN_EN1;
ValeurCmp = CONN_2X2;
IdModule  = pin_array:PIN_ARRAY_2X2;
EndCmp

BeginCmp
TimeStamp = /47D80202/46540159;
Reference = CAN_TERM1;
ValeurCmp = JUMPER;
IdModule  = pin_array:PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /461BB62E;
Reference = CLK0;
ValeurCmp = JUMPER;
IdModule  = pin_array:PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /461BB648;
Reference = CLK1;
ValeurCmp = JUMPER;
IdModule  = pin_array:PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /461BB894;
Reference = CLKOUT1;
ValeurCmp = CONN_1;
IdModule  = connect:PINTST;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652BADD;
Reference = COM_SEL1;
ValeurCmp = CONN_3;
IdModule  = pin_array:PIN_ARRAY_3X1;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652BAD4;
Reference = COM_SEL2;
ValeurCmp = CONN_3;
IdModule  = pin_array:PIN_ARRAY_3X1;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652BA65;
Reference = COM_SEL3;
ValeurCmp = CONN_3;
IdModule  = pin_array:PIN_ARRAY_3X1;
EndCmp

BeginCmp
TimeStamp = /46545507;
Reference = CT1;
ValeurCmp = JUMPER;
IdModule  = pin_array:PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /46237F86;
Reference = D1;
ValeurCmp = BAT54;
IdModule  = lib_smd:ST23AK#1;
EndCmp

BeginCmp
TimeStamp = /4623846D;
Reference = D3;
ValeurCmp = BAT54;
IdModule  = lib_smd:ST23AK#1;
EndCmp

BeginCmp
TimeStamp = /47D80202/465306C8;
Reference = D7;
ValeurCmp = 1N4004;
IdModule  = discret:D5;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BC4;
Reference = D8;
ValeurCmp = LED;
IdModule  = lib_smd:SM1206POL;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BA8;
Reference = D9;
ValeurCmp = LED;
IdModule  = lib_smd:SM1206POL;
EndCmp

BeginCmp
TimeStamp = /47D80202/46530747;
Reference = F1;
ValeurCmp = FUSE;
IdModule  = lib_smd:FSUPCMS;
EndCmp

BeginCmp
TimeStamp = /462380B8;
Reference = FB1;
ValeurCmp = BEAD;
IdModule  = lib_smd:SM1206;
EndCmp

BeginCmp
TimeStamp = /465FE6C5;
Reference = GND1;
ValeurCmp = CONN_1;
IdModule  = connect:PINTST;
EndCmp

BeginCmp
TimeStamp = /47D80202/465307C6;
Reference = J1;
ValeurCmp = JACK_2P;
IdModule  = connect:JACK_ALIM;
EndCmp

BeginCmp
TimeStamp = /46238092;
Reference = L1;
ValeurCmp = 10uH;
IdModule  = lib_smd:SM1206;
EndCmp

BeginCmp
TimeStamp = /461BE327;
Reference = L2;
ValeurCmp = 10uH;
IdModule  = lib_smd:SM1206;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B0AE;
Reference = LED1;
ValeurCmp = LED;
IdModule  = lib_smd:SM1206POL;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B0B7;
Reference = LED2;
ValeurCmp = LED;
IdModule  = lib_smd:SM1206POL;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B0BB;
Reference = LED3;
ValeurCmp = LED;
IdModule  = lib_smd:SM1206POL;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B0BC;
Reference = LED4;
ValeurCmp = LED;
IdModule  = lib_smd:SM1206POL;
EndCmp

BeginCmp
TimeStamp = /47D80202/46530639;
Reference = LED5;
ValeurCmp = LED;
IdModule  = lib_smd:SM1206POL;
EndCmp

BeginCmp
TimeStamp = /46237E52;
Reference = LEDABRT1;
ValeurCmp = RED;
IdModule  = lib_smd:SM1206POL;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B108;
Reference = LED_EN1;
ValeurCmp = JUMPER;
IdModule  = pin_array:PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /462383E5;
Reference = LV1;
ValeurCmp = DS1818;
IdModule  = discret:TO92-INVERT;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652A4FB;
Reference = MCU_PORT1;
ValeurCmp = CONN_30X2;
IdModule  = pin_array:PIN_ARRAY_30X2;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BA6;
Reference = P1;
ValeurCmp = CONN_6;
IdModule  = pin_array:PIN_ARRAY-6X1;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76EB2;
Reference = P3;
ValeurCmp = CONN_2X2;
IdModule  = pin_array:PIN_ARRAY_2X2;
EndCmp

BeginCmp
TimeStamp = /47D80204/46ADE55A;
Reference = P4;
ValeurCmp = CONN_20X2;
IdModule  = pin_array:PIN_ARRAY_20X2;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652BF26;
Reference = PULUPEN1;
ValeurCmp = CONN_4X2;
IdModule  = pin_array:pin_array_4x2;
EndCmp

BeginCmp
TimeStamp = /46238519;
Reference = Q1;
ValeurCmp = 3906;
IdModule  = lib_smd:SOT23EBC;
EndCmp

BeginCmp
TimeStamp = /462389B6;
Reference = R1;
ValeurCmp = 1M;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BB661;
Reference = R2;
ValeurCmp = 4,7K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BE039;
Reference = R4;
ValeurCmp = 10K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BE041;
Reference = R5;
ValeurCmp = 10K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BE046;
Reference = R6;
ValeurCmp = 10K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46237E28;
Reference = R7;
ValeurCmp = 1K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BE047;
Reference = R8;
ValeurCmp = 10K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BE230;
Reference = R9;
ValeurCmp = 0;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BE04B;
Reference = R10;
ValeurCmp = 10K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BE051;
Reference = R11;
ValeurCmp = 10K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46237E2F;
Reference = R12;
ValeurCmp = 20K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BE054;
Reference = R13;
ValeurCmp = 10K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46237E3D;
Reference = R14;
ValeurCmp = 270;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /4623847B;
Reference = R15;
ValeurCmp = 4,7K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BAF5C;
Reference = R16;
ValeurCmp = 4,7K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BB790;
Reference = R17;
ValeurCmp = 4,7K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BB795;
Reference = R18;
ValeurCmp = 4,7K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BB798;
Reference = R19;
ValeurCmp = 4,7K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BB799;
Reference = R20;
ValeurCmp = 4,7K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46238545;
Reference = R21;
ValeurCmp = 4,7K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /4623857F;
Reference = R22;
ValeurCmp = 270;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B5F4;
Reference = R23;
ValeurCmp = 10K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BB65F;
Reference = R25;
ValeurCmp = 4,7K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BB8C0;
Reference = R26;
ValeurCmp = 10K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B061;
Reference = R28;
ValeurCmp = 270;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B9D5;
Reference = R30;
ValeurCmp = 10K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B067;
Reference = R31;
ValeurCmp = 270;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B069;
Reference = R32;
ValeurCmp = 270;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B06A;
Reference = R33;
ValeurCmp = 270;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B111;
Reference = R34;
ValeurCmp = 10K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B9CC;
Reference = R35;
ValeurCmp = 10K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/46540063;
Reference = R36;
ValeurCmp = 1K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/46540164;
Reference = R38;
ValeurCmp = 62;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BE50C;
Reference = R45;
ValeurCmp = 4,7K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /461BB742;
Reference = R46;
ValeurCmp = 22;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652BF65;
Reference = R47;
ValeurCmp = 4,7K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652BF62;
Reference = R48;
ValeurCmp = 4,7K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652BF5C;
Reference = R49;
ValeurCmp = 4,7K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652BF48;
Reference = R50;
ValeurCmp = 4,7K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/46530638;
Reference = R53;
ValeurCmp = 270;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BCA;
Reference = R57;
ValeurCmp = 4K7;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BC3;
Reference = R62;
ValeurCmp = 1K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/46A76BA7;
Reference = R63;
ValeurCmp = 1K;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80204/4791D59D;
Reference = R64;
ValeurCmp = 3,3;
IdModule  = discret:R4;
EndCmp

BeginCmp
TimeStamp = /47D80202/4654018B;
Reference = RCAN1;
ValeurCmp = R;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /47D80202/46540184;
Reference = RCAN2;
ValeurCmp = R;
IdModule  = lib_smd:SM0805;
EndCmp

BeginCmp
TimeStamp = /46238597;
Reference = RED1;
ValeurCmp = LED_RESET1;
IdModule  = lib_smd:SM1206POL;
EndCmp

BeginCmp
TimeStamp = /47D80202/4654007F;
Reference = RS1;
ValeurCmp = CONN_1;
IdModule  = connect:PINTST;
EndCmp

BeginCmp
TimeStamp = /465451D4;
Reference = RST_SW1;
ValeurCmp = SW_PUSH;
IdModule  = discret:SW_PUSH_SMALL;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652DDDF;
Reference = SW1;
ValeurCmp = SW_PUSH;
IdModule  = discret:SW_PUSH_SMALL;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652DDE7;
Reference = SW2;
ValeurCmp = SW_PUSH;
IdModule  = discret:SW_PUSH_SMALL;
EndCmp

BeginCmp
TimeStamp = /47D80202/46530763;
Reference = SW_ONOFF1;
ValeurCmp = SWITCH_INV;
IdModule  = discret:SW_SPDT;
EndCmp

BeginCmp
TimeStamp = /461BBA34;
Reference = TA-1;
ValeurCmp = CONN_1;
IdModule  = connect:PINTST;
EndCmp

BeginCmp
TimeStamp = /47D80202/46530806;
Reference = TB1;
ValeurCmp = CONN_2;
IdModule  = connect:bornier2;
EndCmp

BeginCmp
TimeStamp = /46161C39;
Reference = U1;
ValeurCmp = MCF5213-LQFP100;
IdModule  = lib_smd:VQFP100;
EndCmp

BeginCmp
TimeStamp = /46554FB5;
Reference = U2;
ValeurCmp = 74AHC1G14;
IdModule  = lib_smd:SOT353;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B22B;
Reference = U3;
ValeurCmp = MAX202;
IdModule  = lib_smd:SO16E;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B03E;
Reference = U4;
ValeurCmp = 74HC125;
IdModule  = lib_smd:SO14E;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4C1;
Reference = U5;
ValeurCmp = MAX202;
IdModule  = lib_smd:SO16E;
EndCmp

BeginCmp
TimeStamp = /47D80202/4653FF97;
Reference = U7;
ValeurCmp = PCA82C251;
IdModule  = lib_smd:SO8E;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4D3;
Reference = U8;
ValeurCmp = MAX202;
IdModule  = lib_smd:SO16E;
EndCmp

BeginCmp
TimeStamp = /47D80204/470F38BE;
Reference = U9;
ValeurCmp = XCR3256-TQ144;
IdModule  = lib_smd:TQFP144;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B26D;
Reference = UARTCAN0;
ValeurCmp = DB9;
IdModule  = connect:DB9FC;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4C2;
Reference = UARTCAN1;
ValeurCmp = DB9;
IdModule  = connect:DB9FC;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4D4;
Reference = UARTCAN2;
ValeurCmp = DB9;
IdModule  = connect:DB9FC;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B289;
Reference = UART_EN0;
ValeurCmp = CONN_4X2;
IdModule  = pin_array:pin_array_4x2;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4C3;
Reference = UART_EN1;
ValeurCmp = CONN_4X2;
IdModule  = pin_array:pin_array_4x2;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652B4D5;
Reference = UART_EN2;
ValeurCmp = CONN_4X2;
IdModule  = pin_array:pin_array_4x2;
EndCmp

BeginCmp
TimeStamp = /46238079;
Reference = VDDA1;
ValeurCmp = JUMPER;
IdModule  = pin_array:PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /47D80202/46603376;
Reference = VR1;
ValeurCmp = LT1129_QPACK;
IdModule  = lib_smd:DPAK5;
EndCmp

BeginCmp
TimeStamp = /47D80202/4654003D;
Reference = VREF1;
ValeurCmp = CONN_1;
IdModule  = connect:PINTST;
EndCmp

BeginCmp
TimeStamp = /47D80202/4652A9C4;
Reference = VX_EN1;
ValeurCmp = JUMPER;
IdModule  = pin_array:PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /462389C7;
Reference = Y1;
ValeurCmp = 8MHz;
IdModule  = discret:HC-18UH;
EndCmp

EndListe
