(export (version D)
  (design
    (source F:/kicad-launchpad/testing/demos/ecc83/ecc83-pp.sch)
    (date "04/07/2014 20:15:10")
    (tool "Eeschema (2014-07-02 BZR 4969)-product"))
  (components
    (comp (ref U1)
      (value ECC83)
      (footprint VALVE-NOVAL_P)
      (libsource (lib valves) (part ECC83))
      (sheetpath (names /) (tstamps /))
      (tstamp 48B4F266))
    (comp (ref P4)
      (value CONN_2)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 456A8ACC))
    (comp (ref C1)
      (value 10uF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4549F4BE))
    (comp (ref P3)
      (value POWER)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 4549F4A5))
    (comp (ref P2)
      (value OUT)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 4549F46C))
    (comp (ref P1)
      (value IN)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 4549F464))
    (comp (ref C2)
      (value 680nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4549F3BE))
    (comp (ref R3)
      (value 100K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4549F3AD))
    (comp (ref R4)
      (value 47K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4549F3A2))
    (comp (ref R2)
      (value 1.5K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4549F39D))
    (comp (ref R1)
      (value 1.5K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4549F38A)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib valves) (part ECC81)
      (aliases
        (alias ECC83))
      (fields
        (field (name Reference) U)
        (field (name Value) ECC81)
        (field (name Footprint) VALVE-NOVAL_P))
      (pins
        (pin (num 1) (name A) (type output))
        (pin (num 2) (name G) (type input))
        (pin (num 3) (name K) (type BiDi))
        (pin (num 4) (name F1) (type power_in))
        (pin (num 5) (name F1) (type power_in))
        (pin (num 6) (name A) (type output))
        (pin (num 7) (name G) (type input))
        (pin (num 8) (name K) (type BiDi))
        (pin (num 9) (name F2) (type power_in)))))
  (libraries
    (library (logical device)
      (uri f:\kicad\share\library\device.lib))
    (library (logical conn)
      (uri f:\kicad\share\library\conn.lib))
    (library (logical valves)
      (uri f:\kicad\share\library\valves.lib)))
  (nets
    (net (code 1) (name "Net-(C1-Pad1)")
      (node (ref U1) (pin 6))
      (node (ref C1) (pin 1))
      (node (ref P3) (pin 1)))
    (net (code 2) (name "Net-(R2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref U1) (pin 3)))
    (net (code 3) (name "Net-(C2-Pad2)")
      (node (ref U1) (pin 8))
      (node (ref R1) (pin 2))
      (node (ref C2) (pin 2)))
    (net (code 4) (name "Net-(C2-Pad1)")
      (node (ref C2) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref P2) (pin 1)))
    (net (code 5) (name "Net-(P4-Pad2)")
      (node (ref U1) (pin 9))
      (node (ref P4) (pin 2)))
    (net (code 6) (name "Net-(P1-Pad2)")
      (node (ref U1) (pin 2))
      (node (ref P1) (pin 2))
      (node (ref R4) (pin 1)))
    (net (code 7) (name "Net-(R1-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref U1) (pin 7)))
    (net (code 8) (name GND)
      (node (ref R3) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref P1) (pin 1))
      (node (ref P2) (pin 2))
      (node (ref P3) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref R2) (pin 2)))
    (net (code 9) (name "Net-(P4-Pad1)")
      (node (ref U1) (pin 4))
      (node (ref U1) (pin 5))
      (node (ref P4) (pin 1)))))