(export (version D)
  (design
    (source F:/kicad-launchpad/testing/demos/complex_hierarchy/complex_hierarchy.sch)
    (date "25/01/2014 08:31:41")
    (tool "eeschema (2014-01-22 BZR 4630)-product"))
  (components
    (comp (ref C10)
      (value 10uF)
      (fields)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 4B4B15E7))
    (comp (ref C11)
      (value 10uF)
      (fields)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 4B4B15D9))
    (comp (ref U2)
      (value 78L05)
      (libsource (lib regul) (part 7805))
      (sheetpath (names /) (tstamps /))
      (tstamp 4B4B1532))
    (comp (ref U1)
      (value ICL7660)
      (libsource (lib special) (part ICL7660))
      (sheetpath (names /) (tstamps /))
      (tstamp 4B4B1230))
    (comp (ref C9)
      (value 47uF/63V)
      (fields)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 4B3A1558))
    (comp (ref P1)
      (value CONN_2)
      (fields)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 4B3A12F4))
    (comp (ref C1)
      (value 47uF)
      (fields)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 4B03CEC2))
    (comp (ref C2)
      (value 47uF/20V)
      (fields)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 4AE173CF))
    (comp (ref D1)
      (value 1N4007)
      (fields)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /) (tstamps /))
      (tstamp 4AE172F4))
    (comp (ref P2)
      (value CONN_2)
      (fields)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 4AD71B06))
    (comp (ref R28)
      (value 220K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B617B88))
    (comp (ref R27)
      (value 47)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B616B96))
    (comp (ref D9)
      (value 1N4148)
      (fields)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B616AFA))
    (comp (ref R20)
      (value 5,6K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B61688C))
    (comp (ref C14)
      (value 150nF)
      (libsource (lib device) (part C))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B4F3641))
    (comp (ref R24)
      (value 1K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B4F363E))
    (comp (ref Q6)
      (value MPAS42)
      (fields)
      (libsource (lib transistors) (part MPSA42))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A137D))
    (comp (ref Q7)
      (value MPAS92)
      (fields)
      (libsource (lib transistors) (part MPSA92))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A137C))
    (comp (ref D7)
      (value 1N4148)
      (fields)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A137B))
    (comp (ref Q8)
      (value MPAS42)
      (fields)
      (libsource (lib transistors) (part MPSA42))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1379))
    (comp (ref D6)
      (value 1N4148)
      (fields)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1377))
    (comp (ref R13)
      (value 470)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1376))
    (comp (ref D5)
      (value 1N4148)
      (fields)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1375))
    (comp (ref R14)
      (value 220K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1374))
    (comp (ref R18)
      (value 1K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1371))
    (comp (ref R22)
      (value 220K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1370))
    (comp (ref R19)
      (value 1K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A136D))
    (comp (ref P5)
      (value CONN_2)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A136C))
    (comp (ref R16)
      (value 22K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A136B))
    (comp (ref U4)
      (value LM358N)
      (libsource (lib linear) (part LM358N))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1368))
    (comp (ref P6)
      (value CONN_2)
      (fields)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1367))
    (comp (ref C7)
      (value 4,7nF)
      (libsource (lib device) (part C))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1366))
    (comp (ref C8)
      (value 820pF)
      (libsource (lib device) (part C))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1365))
    (comp (ref R15)
      (value 47)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1364))
    (comp (ref R21)
      (value 4,7K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1362))
    (comp (ref Q5)
      (value MPAS92)
      (fields)
      (libsource (lib transistors) (part MPSA92))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1360))
    (comp (ref R17)
      (value 22K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1359))
    (comp (ref C6)
      (value 15nF)
      (libsource (lib device) (part C))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1358))
    (comp (ref RV2)
      (value 4,7K)
      (libsource (lib device) (part POT))
      (sheetpath (names /ampli_ht_horizontal/) (tstamps /4B3A13A4/))
      (tstamp 4B3A1357))
    (comp (ref R26)
      (value 220K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B617B88))
    (comp (ref R25)
      (value 47)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B616B96))
    (comp (ref D8)
      (value 1N4148)
      (fields)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B616AFA))
    (comp (ref R10)
      (value 5,6K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B61688C))
    (comp (ref C12)
      (value 150nF)
      (libsource (lib device) (part C))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B4F3641))
    (comp (ref R23)
      (value 1K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B4F363E))
    (comp (ref Q2)
      (value MPAS42)
      (fields)
      (libsource (lib transistors) (part MPSA42))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A137D))
    (comp (ref Q3)
      (value MPAS92)
      (fields)
      (libsource (lib transistors) (part MPSA92))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A137C))
    (comp (ref D4)
      (value 1N4148)
      (fields)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A137B))
    (comp (ref Q4)
      (value MPAS42)
      (fields)
      (libsource (lib transistors) (part MPSA42))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1379))
    (comp (ref D3)
      (value 1N4148)
      (fields)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1377))
    (comp (ref R3)
      (value 470)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1376))
    (comp (ref D2)
      (value 1N4148)
      (fields)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1375))
    (comp (ref R4)
      (value 220K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1374))
    (comp (ref R8)
      (value 1K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1371))
    (comp (ref R12)
      (value 220K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1370))
    (comp (ref R9)
      (value 1K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A136D))
    (comp (ref P3)
      (value CONN_2)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A136C))
    (comp (ref R6)
      (value 22K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A136B))
    (comp (ref U3)
      (value LM358N)
      (libsource (lib linear) (part LM358N))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1368))
    (comp (ref P4)
      (value CONN_2)
      (fields)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1367))
    (comp (ref C4)
      (value 4,7nF)
      (libsource (lib device) (part C))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1366))
    (comp (ref C5)
      (value 820pF)
      (libsource (lib device) (part C))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1365))
    (comp (ref R5)
      (value 47)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1364))
    (comp (ref R11)
      (value 4,7K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1362))
    (comp (ref Q1)
      (value MPAS92)
      (fields)
      (libsource (lib transistors) (part MPSA92))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1360))
    (comp (ref R7)
      (value 22K)
      (fields)
      (libsource (lib device) (part R))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1359))
    (comp (ref C3)
      (value 15nF)
      (libsource (lib device) (part C))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1358))
    (comp (ref RV1)
      (value 4,7K)
      (libsource (lib device) (part POT))
      (sheetpath (names /ampli_ht_vertical/) (tstamps /4B3A1333/))
      (tstamp 4B3A1357)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP)
      (aliases
        (alias CAPAPOL))
      (description "Condensateur polarise")
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part DIODE)
      (description "Diode simple")
      (footprints
        (fp D?)
        (fp S*))
      (fields
        (field (name Reference) D)
        (field (name Value) DIODE))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part POT)
      (description Potentionmetre)
      (fields
        (field (name Reference) RV)
        (field (name Value) POT))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib transistors) (part MPSA42)
      (description "MPSA42, Vce 300V, Ic 500mA, NPN High Voltage Transistor")
      (docs transistors/bipolar/MPSA42.pdf)
      (footprints
        (fp TO92-CBE))
      (fields
        (field (name Reference) Q)
        (field (name Value) MPSA42)
        (field (name Footprint) TO92-CBE))
      (pins
        (pin (num B) (name B) (type input))
        (pin (num C) (name C) (type passive))
        (pin (num E) (name E) (type passive))))
    (libpart (lib transistors) (part MPSA92)
      (description "MPSA92, Vce 300V, Ic 500mA, PNP High Voltage Transistor")
      (docs transistors/bipolar/mpsa92.pdf)
      (footprints
        (fp TO92-CBE))
      (fields
        (field (name Reference) Q)
        (field (name Value) MPSA92)
        (field (name Footprint) TO92-CBE))
      (pins
        (pin (num B) (name B) (type input))
        (pin (num C) (name C) (type passive))
        (pin (num E) (name E) (type passive))))
    (libpart (lib conn) (part CONN_2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib linear) (part LM358)
      (aliases
        (alias LMC6062)
        (alias LMC6082)
        (alias LM358N)
        (alias TL072)
        (alias TL082))
      (description "Dual Op amp (low power)")
      (docs ns/lm158.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) LM358))
      (pins
        (pin (num 1) (name ~) (type output))
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V-) (type power_in))
        (pin (num 5) (name +) (type input))
        (pin (num 6) (name -) (type input))
        (pin (num 7) (name ~) (type output))
        (pin (num 8) (name V+) (type power_in))))
    (libpart (lib regul) (part 7805)
      (aliases
        (alias LM7805)
        (alias LM7812)
        (alias 78L05))
      (description "Linear Regulator +5V")
      (docs regulator\lm78xx.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) 7805))
      (pins
        (pin (num GND) (name GND) (type input))
        (pin (num VI) (name VI) (type input))
        (pin (num VO) (name VO) (type power_out))))
    (libpart (lib special) (part ICL7660)
      (description "Voltage converter (pump)")
      (docs intersil/icl7660.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) ICL7660))
      (pins
        (pin (num 2) (name CAP+) (type input))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name CAP-) (type input))
        (pin (num 5) (name VOUT) (type power_out))
        (pin (num 6) (name LV) (type input))
        (pin (num 7) (name OSC) (type input))
        (pin (num 8) (name V+) (type power_in)))))
  (libraries
    (library (logical device)
      (uri F:\kicad\share\library\device.lib))
    (library (logical transistors)
      (uri F:\kicad\share\library\transistors.lib))
    (library (logical conn)
      (uri F:\kicad\share\library\conn.lib))
    (library (logical linear)
      (uri F:\kicad\share\library\linear.lib))
    (library (logical regul)
      (uri F:\kicad\share\library\regul.lib))
    (library (logical special)
      (uri F:\kicad\share\library\special.lib)))
  (nets
    (net (code 1) (name HT)
      (node (ref Q2) (pin C))
      (node (ref R13) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref Q6) (pin C))
      (node (ref D5) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref P1) (pin 1)))
    (net (code 2) (name GND)
      (node (ref C11) (pin 1))
      (node (ref C12) (pin 2))
      (node (ref Q7) (pin C))
      (node (ref C8) (pin 2))
      (node (ref P6) (pin 2))
      (node (ref R21) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref P3) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref P4) (pin 2))
      (node (ref Q3) (pin C))
      (node (ref C2) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref P2) (pin 2))
      (node (ref R18) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref U1) (pin 3))
      (node (ref R4) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref P1) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref P5) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref U2) (pin GND))
      (node (ref C5) (pin 2)))
    (net (code 3) (name "Net-(U1-Pad7)")
      (node (ref U1) (pin 7)))
    (net (code 4) (name "Net-(U1-Pad6)")
      (node (ref U1) (pin 6)))
    (net (code 5) (name "Net-(C10-Pad2)")
      (node (ref C10) (pin 2))
      (node (ref U1) (pin 4)))
    (net (code 6) (name "Net-(C10-Pad1)")
      (node (ref U1) (pin 2))
      (node (ref C10) (pin 1)))
    (net (code 7) (name /12Vext)
      (node (ref P2) (pin 1))
      (node (ref D1) (pin 1)))
    (net (code 8) (name +12V)
      (node (ref U3) (pin 8))
      (node (ref C2) (pin 1))
      (node (ref D1) (pin 2))
      (node (ref U2) (pin VI))
      (node (ref U4) (pin 8)))
    (net (code 9) (name VCC)
      (node (ref U1) (pin 8))
      (node (ref C1) (pin 1))
      (node (ref U2) (pin VO)))
    (net (code 10) (name -VAA)
      (node (ref U3) (pin 4))
      (node (ref U4) (pin 4))
      (node (ref U1) (pin 5))
      (node (ref C11) (pin 2)))
    (net (code 11) (name "Net-(Q4-PadE)")
      (node (ref Q4) (pin E))
      (node (ref R9) (pin 1)))
    (net (code 12) (name "Net-(Q3-PadE)")
      (node (ref R25) (pin 2))
      (node (ref Q3) (pin E))
      (node (ref R12) (pin 2)))
    (net (code 13) (name "Net-(D4-Pad2)")
      (node (ref D4) (pin 2))
      (node (ref Q3) (pin B))
      (node (ref Q4) (pin C))
      (node (ref R10) (pin 1)))
    (net (code 14) (name "Net-(D2-Pad2)")
      (node (ref D2) (pin 2))
      (node (ref D3) (pin 1)))
    (net (code 15) (name "Net-(C12-Pad1)")
      (node (ref C12) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref R23) (pin 1)))
    (net (code 16) (name "Net-(C5-Pad1)")
      (node (ref C5) (pin 1))
      (node (ref R10) (pin 2)))
    (net (code 17) (name "Net-(Q2-PadE)")
      (node (ref R5) (pin 2))
      (node (ref Q2) (pin E))
      (node (ref R26) (pin 2)))
    (net (code 18) (name "Net-(D4-Pad1)")
      (node (ref D4) (pin 1))
      (node (ref D8) (pin 2)))
    (net (code 19) (name "Net-(R11-Pad1)")
      (node (ref RV1) (pin 1))
      (node (ref R11) (pin 1)))
    (net (code 20) (name "Net-(D3-Pad2)")
      (node (ref R4) (pin 1))
      (node (ref Q1) (pin B))
      (node (ref D3) (pin 2)))
    (net (code 21) (name "Net-(R9-Pad2)")
      (node (ref U3) (pin 1))
      (node (ref R9) (pin 2)))
    (net (code 22) (name "Net-(RV1-Pad2)")
      (node (ref U3) (pin 2))
      (node (ref RV1) (pin 2)))
    (net (code 23) (name "Net-(C3-Pad2)")
      (node (ref R6) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref R7) (pin 2)))
    (net (code 24) (name "Net-(C4-Pad1)")
      (node (ref U3) (pin 5))
      (node (ref C4) (pin 1))
      (node (ref R7) (pin 1)))
    (net (code 25) (name "Net-(Q4-PadB)")
      (node (ref R8) (pin 1))
      (node (ref Q4) (pin B)))
    (net (code 26) (name "Net-(D8-Pad1)")
      (node (ref Q1) (pin C))
      (node (ref D8) (pin 1))
      (node (ref Q2) (pin B)))
    (net (code 27) (name "Net-(Q1-PadE)")
      (node (ref Q1) (pin E))
      (node (ref R3) (pin 2)))
    (net (code 28) (name /ampli_ht_vertical/Vpil_0_3,3V)
      (node (ref U3) (pin 6))
      (node (ref U3) (pin 7))
      (node (ref C3) (pin 1))
      (node (ref U3) (pin 3)))
    (net (code 29) (name /ampli_ht_vertical/PIEZO_OUT)
      (node (ref R5) (pin 1))
      (node (ref P3) (pin 1))
      (node (ref R25) (pin 1)))
    (net (code 30) (name /ampli_ht_vertical/PIEZO_IN)
      (node (ref P4) (pin 1))
      (node (ref R23) (pin 2)))
    (net (code 31) (name /ampli_ht_vertical/S_OUT+)
      (node (ref RV1) (pin 3))
      (node (ref R12) (pin 1))
      (node (ref R26) (pin 1)))
    (net (code 32) (name "Net-(Q7-PadE)")
      (node (ref R27) (pin 2))
      (node (ref R22) (pin 2))
      (node (ref Q7) (pin E)))
    (net (code 33) (name "Net-(D7-Pad2)")
      (node (ref R20) (pin 1))
      (node (ref D7) (pin 2))
      (node (ref Q8) (pin C))
      (node (ref Q7) (pin B)))
    (net (code 34) (name "Net-(Q8-PadE)")
      (node (ref Q8) (pin E))
      (node (ref R19) (pin 1)))
    (net (code 35) (name "Net-(D5-Pad2)")
      (node (ref D6) (pin 1))
      (node (ref D5) (pin 2)))
    (net (code 36) (name "Net-(C6-Pad2)")
      (node (ref C6) (pin 2))
      (node (ref R17) (pin 2))
      (node (ref R16) (pin 1)))
    (net (code 37) (name "Net-(C14-Pad1)")
      (node (ref C14) (pin 1))
      (node (ref R16) (pin 2))
      (node (ref R24) (pin 1)))
    (net (code 38) (name "Net-(C8-Pad1)")
      (node (ref R20) (pin 2))
      (node (ref C8) (pin 1)))
    (net (code 39) (name "Net-(Q6-PadE)")
      (node (ref Q6) (pin E))
      (node (ref R15) (pin 2))
      (node (ref R28) (pin 2)))
    (net (code 40) (name "Net-(D7-Pad1)")
      (node (ref D9) (pin 2))
      (node (ref D7) (pin 1)))
    (net (code 41) (name "Net-(R21-Pad1)")
      (node (ref RV2) (pin 1))
      (node (ref R21) (pin 1)))
    (net (code 42) (name "Net-(D6-Pad2)")
      (node (ref R14) (pin 1))
      (node (ref D6) (pin 2))
      (node (ref Q5) (pin B)))
    (net (code 43) (name "Net-(R19-Pad2)")
      (node (ref U4) (pin 1))
      (node (ref R19) (pin 2)))
    (net (code 44) (name "Net-(RV2-Pad2)")
      (node (ref RV2) (pin 2))
      (node (ref U4) (pin 2)))
    (net (code 45) (name "Net-(C7-Pad1)")
      (node (ref U4) (pin 5))
      (node (ref R17) (pin 1))
      (node (ref C7) (pin 1)))
    (net (code 46) (name "Net-(Q8-PadB)")
      (node (ref Q8) (pin B))
      (node (ref R18) (pin 1)))
    (net (code 47) (name "Net-(D9-Pad1)")
      (node (ref Q6) (pin B))
      (node (ref Q5) (pin C))
      (node (ref D9) (pin 1)))
    (net (code 48) (name "Net-(Q5-PadE)")
      (node (ref R13) (pin 2))
      (node (ref Q5) (pin E)))
    (net (code 49) (name /ampli_ht_horizontal/Vpil_0_3,3V)
      (node (ref U4) (pin 3))
      (node (ref C6) (pin 1))
      (node (ref U4) (pin 7))
      (node (ref U4) (pin 6)))
    (net (code 50) (name /ampli_ht_horizontal/PIEZO_OUT)
      (node (ref R27) (pin 1))
      (node (ref R15) (pin 1))
      (node (ref P5) (pin 1)))
    (net (code 51) (name /ampli_ht_horizontal/PIEZO_IN)
      (node (ref P6) (pin 1))
      (node (ref R24) (pin 2)))
    (net (code 52) (name /ampli_ht_horizontal/S_OUT+)
      (node (ref R28) (pin 1))
      (node (ref R22) (pin 1))
      (node (ref RV2) (pin 3)))))