(export (version D)
  (design
    (source "F:/kicad-launchpad/testing/demos/sonde xilinx/sonde xilinx.sch")
    (date "05/01/2014 18:35:33")
    (tool "eeschema (2014-01-04 BZR 4608)-product"))
  (components
    (comp (ref R11)
      (value 100)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D527316))
    (comp (ref C4)
      (value 100pF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF81A7))
    (comp (ref R13)
      (value 100)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D528082))
    (comp (ref U1)
      (value 74LS125)
      (libsource (lib 74xx) (part 74LS125))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF7DBD))
    (comp (ref J2)
      (value DB9MALE)
      (libsource (lib conn) (part DB9))
      (sheetpath (names /) (tstamps /))
      (tstamp 3ECDE5C8))
    (comp (ref P1)
      (value CONN_6)
      (libsource (lib conn) (part CONN_6))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF830C))
    (comp (ref C1)
      (value 1uF)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF82C6))
    (comp (ref C5)
      (value 100pF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D528086))
    (comp (ref R12)
      (value 100)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D528083))
    (comp (ref C2)
      (value 100pF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D528085))
    (comp (ref C3)
      (value 100pF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D528084))
    (comp (ref R14)
      (value 100)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF819B))
    (comp (ref R5)
      (value 1K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF818E))
    (comp (ref R2)
      (value 5,1K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF8187))
    (comp (ref D2)
      (value BAT46)
      (libsource (lib device) (part DIODESCH))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF8176))
    (comp (ref D1)
      (value BAT46)
      (libsource (lib device) (part DIODESCH))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF815E))
    (comp (ref U2)
      (value 74LS125)
      (libsource (lib 74xx) (part 74LS125))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF7EEC))
    (comp (ref R9)
      (value 100)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF7D33))
    (comp (ref R10)
      (value 100)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF7D31))
    (comp (ref R8)
      (value 100)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D528080))
    (comp (ref R7)
      (value 100)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D52807F))
    (comp (ref R6)
      (value 100)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF7D26))
    (comp (ref R4)
      (value 47)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF7D22))
    (comp (ref R1)
      (value 100)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF7D16))
    (comp (ref J1)
      (value DB25MALE)
      (libsource (lib conn) (part DB25))
      (sheetpath (names /) (tstamps /))
      (tstamp 3EBF7D04)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP)
      (aliases
        (alias CAPAPOL))
      (description "Condensateur polarise")
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part DIODESCH)
      (description "Diode schottky")
      (footprints
        (fp D?)
        (fp S*))
      (fields
        (field (name Reference) D)
        (field (name Value) DIODESCH))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_6)
      (description "ymbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_6))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))))
    (libpart (lib conn) (part DB25)
      (footprints
        (fp DB25*))
      (fields
        (field (name Reference) J)
        (field (name Value) DB25))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))
        (pin (num 10) (name 10) (type passive))
        (pin (num 11) (name 11) (type passive))
        (pin (num 12) (name 12) (type passive))
        (pin (num 13) (name 13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))))
    (libpart (lib conn) (part DB9)
      (footprints
        (fp DB9*))
      (fields
        (field (name Reference) J)
        (field (name Value) DB9))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))))
    (libpart (lib 74xx) (part 74LS125)
      (description "Quad buffer 3 State out")
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS125))
      (pins
        (pin (num 1) (name E) (type input))
        (pin (num 2) (name D) (type input))
        (pin (num 3) (name O) (type 3state))
        (pin (num 4) (name E) (type input))
        (pin (num 5) (name D) (type input))
        (pin (num 6) (name O) (type 3state))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name O) (type 3state))
        (pin (num 9) (name D) (type input))
        (pin (num 10) (name E) (type input))
        (pin (num 11) (name O) (type 3state))
        (pin (num 12) (name D) (type input))
        (pin (num 13) (name E) (type input))
        (pin (num 14) (name VCC) (type power_in)))))
  (libraries
    (library (logical device)
      (uri F:\kicad\share\library\device.lib))
    (library (logical conn)
      (uri F:\kicad\share\library\conn.lib))
    (library (logical 74xx)
      (uri F:\kicad\share\library\74xx.lib)))
  (nets
    (net (code 1) (name VCC)
      (node (ref U2) (pin 14))
      (node (ref R5) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref D2) (pin 2))
      (node (ref D1) (pin 1))
      (node (ref U1) (pin 14))
      (node (ref C1) (pin 1)))
    (net (code 2) (name GND)
      (node (ref J2) (pin 7))
      (node (ref J2) (pin 8))
      (node (ref J2) (pin 9))
      (node (ref C5) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U1) (pin 7))
      (node (ref J1) (pin 20))
      (node (ref U2) (pin 1))
      (node (ref J1) (pin 25))
      (node (ref U2) (pin 12))
      (node (ref U2) (pin 10))
      (node (ref U2) (pin 9))
      (node (ref U2) (pin 7))
      (node (ref U2) (pin 4))
      (node (ref U2) (pin 5))
      (node (ref P1) (pin 2))
      (node (ref U2) (pin 13))
      (node (ref C3) (pin 2))
      (node (ref J2) (pin 6))
      (node (ref C4) (pin 2))
      (node (ref C2) (pin 2)))
    (net (code 3) (name "Net-(U2-Pad11)")
      (node (ref U2) (pin 11)))
    (net (code 4) (name "Net-(U2-Pad8)")
      (node (ref U2) (pin 8)))
    (net (code 5) (name "Net-(U2-Pad6)")
      (node (ref U2) (pin 6)))
    (net (code 6) (name /TMS-PROG-D2)
      (node (ref J1) (pin 4))
      (node (ref R9) (pin 2)))
    (net (code 7) (name /VCC_SENSE-ERROR*)
      (node (ref J1) (pin 15))
      (node (ref R1) (pin 2)))
    (net (code 8) (name "Net-(J1-Pad11)")
      (node (ref J1) (pin 12))
      (node (ref J1) (pin 11))
      (node (ref J1) (pin 8)))
    (net (code 9) (name /TD0-PROG-D4)
      (node (ref J1) (pin 6))
      (node (ref R6) (pin 2)))
    (net (code 10) (name /TDI-DIN-D0)
      (node (ref J1) (pin 2))
      (node (ref R7) (pin 2)))
    (net (code 11) (name /CTRL-D3)
      (node (ref J1) (pin 5))
      (node (ref R8) (pin 2)))
    (net (code 12) (name /CLK-D1)
      (node (ref J1) (pin 3))
      (node (ref R10) (pin 2)))
    (net (code 13) (name "Net-(R4-Pad1)")
      (node (ref R4) (pin 1))
      (node (ref U2) (pin 3)))
    (net (code 14) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1)))
    (net (code 15) (name "Net-(J1-Pad7)")
      (node (ref J1) (pin 7)))
    (net (code 16) (name "Net-(R7-Pad1)")
      (node (ref U1) (pin 5))
      (node (ref R7) (pin 1)))
    (net (code 17) (name /DONE-SELECT*)
      (node (ref J1) (pin 13))
      (node (ref R4) (pin 2)))
    (net (code 18) (name "Net-(J1-Pad19)")
      (node (ref J1) (pin 19)))
    (net (code 19) (name "Net-(J1-Pad18)")
      (node (ref J1) (pin 18)))
    (net (code 20) (name "Net-(J1-Pad17)")
      (node (ref J1) (pin 17)))
    (net (code 21) (name "Net-(J1-Pad16)")
      (node (ref J1) (pin 16)))
    (net (code 22) (name "Net-(J1-Pad24)")
      (node (ref J1) (pin 24)))
    (net (code 23) (name "Net-(J1-Pad14)")
      (node (ref J1) (pin 14)))
    (net (code 24) (name "Net-(J1-Pad23)")
      (node (ref J1) (pin 23)))
    (net (code 25) (name "Net-(R9-Pad1)")
      (node (ref U1) (pin 12))
      (node (ref R9) (pin 1)))
    (net (code 26) (name "Net-(J1-Pad22)")
      (node (ref J1) (pin 22)))
    (net (code 27) (name "Net-(J1-Pad21)")
      (node (ref J1) (pin 21)))
    (net (code 28) (name "Net-(J1-Pad10)")
      (node (ref J1) (pin 10)))
    (net (code 29) (name "Net-(J1-Pad9)")
      (node (ref J1) (pin 9)))
    (net (code 30) (name "Net-(R10-Pad1)")
      (node (ref R10) (pin 1))
      (node (ref U1) (pin 9)))
    (net (code 31) (name "Net-(R6-Pad1)")
      (node (ref R6) (pin 1))
      (node (ref U1) (pin 1)))
    (net (code 32) (name "Net-(D1-Pad2)")
      (node (ref R1) (pin 1))
      (node (ref D1) (pin 2)))
    (net (code 33) (name "Net-(C4-Pad1)")
      (node (ref C4) (pin 1))
      (node (ref R13) (pin 2))
      (node (ref U1) (pin 11)))
    (net (code 34) (name "Net-(R8-Pad1)")
      (node (ref U1) (pin 4))
      (node (ref R8) (pin 1))
      (node (ref U1) (pin 10))
      (node (ref U1) (pin 13)))
    (net (code 35) (name /PWR_3,3-5V)
      (node (ref D2) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref P1) (pin 1)))
    (net (code 36) (name "Net-(C2-Pad1)")
      (node (ref U1) (pin 6))
      (node (ref C2) (pin 1))
      (node (ref R11) (pin 2)))
    (net (code 37) (name "Net-(C5-Pad1)")
      (node (ref U1) (pin 8))
      (node (ref C5) (pin 1))
      (node (ref R12) (pin 2)))
    (net (code 38) (name "Net-(C3-Pad1)")
      (node (ref R2) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref U2) (pin 2)))
    (net (code 39) (name /TD0-DONE)
      (node (ref P1) (pin 3))
      (node (ref J2) (pin 2))
      (node (ref R14) (pin 1)))
    (net (code 40) (name /TDI-DIN)
      (node (ref P1) (pin 4))
      (node (ref R11) (pin 1))
      (node (ref J2) (pin 3)))
    (net (code 41) (name /TCK-CCLK)
      (node (ref P1) (pin 5))
      (node (ref R12) (pin 1))
      (node (ref J2) (pin 4)))
    (net (code 42) (name /TMS-PROG)
      (node (ref J2) (pin 5))
      (node (ref P1) (pin 6))
      (node (ref R13) (pin 1)))))